Spec Climate-60

Frequency Response

63 Hz — 30 kHz

Sensitivity (1W@1M)

88 dB

Nominal Impedance

8 ohms

Maximum SPL

108.8 dBa

Power Handling (RMS)

100 W

Recommended Amplifier Requirements

15 — 100 W

Drivers

1 x 165 mm (6 1/2") C-CAM bass/ mid-range driver
1 x 25 mm (1") C-CAM [**Gold Dome tweeter**](https://www.monitoraudio.com/en/blog/introducing-gold-dome-tweeters/)

External Dimensions (H x W x D)

325 x 185 x 178.5 mm (1213/16 x 75/16x 7")

Overall Depth (Including Bracket)

235 mm (91/4")

Total Bracket Pivot Angle

87.5 degrees (from central position)

Fixed Angled Block (Portrait)

15 degrees

Connection

Gold plated 'push' type terminals

Environmental Protection Rating

IP55

Colour / Finish

White/Black

Weight (packaged)

4.62 kg (10 lb 2 oz)